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NEWNAN UTILITIES CONSTRUCTION REQUIREMENTS
RESIDENTIAL / COMMERCIAL
General Notes
1. Newnan Utilities request that the Developer/Owner/Builder/Contractor and/or Engineer discuss service needed prior to plan submittal, construction or remodel.
2. When submitting plans see Design Plan Submittal Section.
3. The Developer/Owner/Builder/Contractor shall submit plans through the City of Newnan and notify Newnan Utilities that plans have been submitted.
4. If construction has not begun within 6 months since plans have been approved or has stopped work more than 1 month, the Developer/Owner/Builder/Contractor shall notify Newnan Utilities.
5. The Developer/Owner/Builder/Contractor shall contact Terry Brown for residential lot construction or remodel 48 hours prior to work starting at (404) 461-3399.
6. The Developer/Owner/Builder/Contractor shall contact Scott Tolar 48 hours for all commercial, residential construction other than individual lots, commercial remodels at (770) 301-0245
7. Newnan Utilities requires an open ditch inspection of both water and sanitary sewer service/main prior to covering up.
8. To schedule a residential open ditch and final inspection the Developer/Owner/Builder /Contractor shall complete the form located on Newnan Utilities Website under Wastewater tab/Line Inspection.
9. It is the responsibility of the Developer/Owner/Builder/Contractor to verify all utility locations prior to start of work.  They are responsible to notify Georgia 811.
10. Developer/Owner/Builder/Contractor shall be responsible for protecting all utility services lines and laterals, both municipal and owner side of the services during construction.
11. If any damage is found to service both municipal side and owner side, prior to, during construction, or after construction, it shall be the responsibility of the Developer/Owner/Builder to repair prior to final acceptance.
12. The Developer/Owner/Builder shall provide a 2-year warranty on all Water and Sewer Mains.  This warranty period begins when final plat/as-builts have been accepted.  Also, all services shall be warranty up to Certificate of Occupancy.
13. No system shall be accepted, nor shall the warranty period begin until as-builts and final plat are accepted and approved.
14. Only a Current License Utility Contractor shall install water and sanitary sewer mains.
15. All Materials shall be new and manufactures approved by Newnan Utilities
16. No Utility services shall be installed until mains have been excepted.
17. All roads shall have 5-foot utility easements outside of the right-of-way.
18. Newnan Utilities requires backfilling, with clean, suitable acceptable material be used that will compact and provide stability and meet environmental and project specifications.  It shall not contain organic debris, hazardous material, or chemical pollutants that could leach or cause odors.  It should be free of liquids (even water) to avoid slurry formation. 
19. All Water System improvements shall comply with the Georgia EPD Minimum Standards for Public Water System – March 2021 or latest edition.  Newnan Utilities require all water mains 4 inch and large to be class 50 ductile iron pipe.
20. Thrust blocking or approved restraint system shall be installed as required for all pressure pipe installations.
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